Meteorological station

Documentation & report

Date: 15.04.2019

Information Technology

Monday 10:15, group 9

IFE, 4th semester

# Team & task assignment

|  |  |
| --- | --- |
| Piotr Kaźmierski (leader) | * Bluetooth + UART |
| * temperature & humidity sensor |
| Piotr Kocik | * button + interrupts |
| Michał Kuśmidrowicz | * LCD screen + I2C |
| Kacper Kubicki | * pressure sensor + SPI |
| * LED + PWM |

# Devices

* Arduino Uno Rev3
* DHT11 temperature & humidity sensor
* BMP280 temperature, pressure & altitude sensor
* Green LCD 2x16 with LED backlight through a I2C converter
* HC-05 Bluetooth module
* RGB LED
* Tact Switch 6x6mm / 4,3mm THT

# Project description

## General description

The aim of the project was to create a meteorological station which could display the information relating to the weather conditions using an LCD screen with the ability to change currently shown information via a button or remotely, via Bluetooth. Additionally we wanted to add a persistent indicator of a specific weather condition in the form of an RGB LED diode.

## Information to be displayed

Each reading/information is displayed separately, centred on the LCD screen with a heading that informs which mode is currently used, e.g.:

**TEMPERATURE**

**28°C**

Possible information to be displayed are:

* Temperature
* Heat index (perceived temperature)
* Atmospheric pressure

## How to use it?

The currently displayed information can be changed via interrupt driven button (tactile switch) or remotely via Bluetooth using for example a smartphone with an appropriate app installed. The button allows to loop through all the screens one by one in a forward manner. Bluetooth allows to go back and forth between the screens as well as read the data remotely repeatedly or on demand.

### Control using Bluetooth


To use the meteorological station via Bluetooth one must have a Bluetooth enabled device with an app that can perform serial communication via Bluetooth. In our case we’re using “Bluetooth Electronics” by keuwlsoft which is available for Android devices via Google Play. It allows users to send commands via a serial terminal emulator and assign specific terminal commands to buttons and sliders, which makes controlling the device remotely even easier.

**//TUTAJ SCREENSHOTY Z APLIKACJI I JAKIŚ DOKŁADNIEJSZY OPIS**

# Peripherals and interface configuration

## GPIO

Below the GPIO connection diagram is presented:



The table below presents the pinout:

|  |  |  |  |
| --- | --- | --- | --- |
| Pin | Alias | PWM | Assigned to |
| 0 | RX | No | Bluetooth module TX |
| 1 | TX | No | Bluetooth module RX |
| 2 | IRQ0 | No | Tactile switch (interrupt enabled) |
| 3 | IRQ1 | Yes | RBG LED red component |
| 4 | - | No | - |
| 5 | - | Yes | RGB LED green component |
| 6 | - | Yes | RGB LED blue component |
| 7 | - | No | DHT11 data pin |
| 8 | - | No | - |
| 9 | - | Yes | - |
| 10 | SS | Yes | BMP280 CSB pin |
| 11 | MOSI | Yes | BMP280 SDA pin |
| 12 | MISO | No | BMP280 SDO pin |
| 13 | SCK | No | BMP280 SCL pin |
| 14 | A0 | N/A | - |
| 15 | A1 | N/A | - |
| 16 | A2 | N/A | - |
| 17 | A3 | N/A | - |
| 18 | A4, SDA | N/A | I2C LCD converter SDA pin |
| 19 | A5, SCL | N/A | I2C LCD converter SCL pin |

Pins 0 to 13 are digital pins. Some of them are PWM.

Pins A0 to A5 are analogue pins.

Pins 0 and 1 are used for UART communication via the Bluetooth module.

Pin 2, which is assigned to interrupt 0 (IRQ0) is used for the tactile switch.

Pins 3, 5, and 6 are used for red, green and blue components of the RGB diode respectively.

Pin 7 is used for the DHT11 sensor data send & receive.

Pins 10 through 13 are used for SPI communication with the BMP280 sensor.

Pins A4 and A5 are used as SDA and SCL in I2C protocol to communicate with the I2C LCD converter

Some of the pins are configured by the library functions, such as SPI pins, I2C pins and DHT11 pin.

### DHT11

DHT11 is configured using the library functions:

//meteo.ino - our code

#define DHTPIN 7

#define DHTTYPE DHT11

DHT dht(DHTPIN, DHTTYPE);

void setup() {

//...

dht.begin();

//...

}

//DHT.cpp - DHT11 library

void DHT::begin(uint8\_t usec) { //the declaration has a default value for usec set

//...

pinMode(\_pin, INPUT\_PULLUP); //\_pin is a variable set by the DHT constructor that corresponds to the first constructor arugment (in our case DHTPIN that equals 7)

//...

}

An equivalent direct way of doing it is:

pinMode(DHTPIN, INPUT\_PULLUP);

Doing it via directly setting registers:

DDRD |= B10000000; //sets pin 7 to INPUT

PORTD |= B10000000; //sets pin 7 to HIGH, enabling pullup resistors

INPUT\_PULLUP sets a pin into an input mode with a pullup resistor attached. This reverses the way input should be read, since now high voltage = 0, and low voltage = 1.

### USART

USART pins don’t have to be configured.

## I2C

## SPI

## USART

USART is configured via library function call:

const int DEFAULT\_BAUD\_RATE = 9600;

void setup() {

Serial.begin(DEFAULT\_BAUD\_RATE);

//...

}

To configure USART via register manipulation we have to enable the receiver and transmitter, as well as set the baud rate.

UCSR0B = (1<<RXEN0)|(1<<TXEN0); //enables the receiver and transmitter

UBRR0L = 103; //sets the baud rate to 9600

The rest of the settings are kept at default values and the most important of those are:

* Mode of operation: asynchronous
* Parity: disabled
* Stop bits: 1
* Character size: 8 bits

## Interrupts

## PWM

# Failure Mode and Effect Analysis

Some components of the device are of the highest importance – without them, the device cannot fulfil its basic function. However, failure of some other components does not render the whole device unusable. Some components’ importance is context-dependent. In the table below there are a few items and functions which will be considered in failure analysis. In the left column there is the item name, and in the right column the gravity of this item’s failure.

|  |  |
| --- | --- |
| **Item/function** | **Importance** |
| Microcontroller | critical |
| Power supply | critical |
| Screen | low / critical |
| Button | low / critical |
| Bluetooth module | low / critical |
| Temperature and humidity sensor | high |
| Pressure sensor | high |
| LED | low |

The microcontroller and power supply are essential to device’s functioning. The microcontroller is responsible for the program logic and controlling the devices, therefore it cannot fail. Because the device does not have a battery power supply must be constantly available.

The low / critical importance stems from the fact that we can read data and change the currently displayed information in a few ways:

* Changing
  + Using a button
  + Via Bluetooth using an app
* Displaying
  + On the LCD screen
  + In the terminal (via Bluetooth using an app)

Therefore, one way of changing the displayed information can fail, as well as one way of changing the displayed information. However, if both fail, the device wouldn’t be able to function properly: worst case scenario is that nothing is displayed (Bluetooth & screen fail) or we’re stuck on a given mode (button and Bluetooth fail).

The sensors are of high importance since they provide all the data to be displayed. Without them, the data would be either unavailable or “frozen”, that is the reading would always be the same.

LED is of the lowest importance – it only serves as an indicator of one value and it does not affect other components in any way. Moreover, it can be replaced by just adding another mode that would display the reading normally indicated by the LED.

Power supply failure can be detected in a number of ways, for example the LED or screen may flicker. Power‐related faults may also arise when a short in the system is caused, for example from power rail to ground. This may happen either by putting a jumper in the incorrect place, or dropping a piece of metal on the board.

A microcontroller failure would probably be easy to detect, as most likely it would be a complete failure of the chip, not just a small part of the chip.

Screen’s failure would be easily noticeable, since it would either have problems with backlight or displaying the content properly.

Button’s failure might result in fake presses or no reaction when pressed. That would be easy to notice since the screen would change by itself (fake presses) or stay the same even if the button was pressed.

Bluetooth module’s failure could have multiple symptoms, for example the device could disconnect spontaneously, the communication could stop working and so on.

Sensors could stop responding altogether or start giving wrong readings. The 2nd symptom could be hard to realise if the error would be small, unless we had other, reference sensors.

LED’s failure might not be so obvious, since it could also be a power supply failure. Nevertheless, if the LED started shining more dimly or stopped shining altogether it could be sign that it has been damaged.

All of the components could be easily replaced by just swapping them, since they’re connected to the breadboard. The microcontroller is socketed, so it too could be easily replaced. In case of power supply failure the whole component would have to be replaced or if the problem is with the board, the quickest way would be to replace it whole.

# References

* ATmega328P Datasheet (<http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328PB-Automotive-Data-Sheet-40001980B.pdf>)
* DHT11 Datasheet (<https://www.mouser.com/ds/2/758/DHT11-Technical-Data-Sheet-Translated-Version-1143054.pdf>)
* BMP280 Datasheet (<https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BMP280-DS001.pdf>)
* HC-05 Datasheet (<http://www.electronicaestudio.com/docs/istd016A.pdf>)
* HD44780 Datasheet (<https://www.sparkfun.com/datasheets/LCD/HD44780.pdf>)
* Arduino reference materials:
  + Port manipulation: <https://www.arduino.cc/en/Reference/PortManipulation>
  + Digital pins use guide: <https://www.arduino.cc/en/Tutorial/DigitalPins>

# Other information